Cobolt
Speechmaster

Single Induction Hob

Instructions

INTRODUCTION
Thank you for purchasing a Cobolt Speechmaster Talking Induction Hob.  Please take a few moments to read these instructions, particularly those on INSTALLATION and the WARNINGS & SAFETY PRECAUTIONS, before you connect your oven to the power supply.
INSTALLATION
1.  Remove all packing materials and accessories and retain them, in case you need to return the hob to us in the future.
2.  Place the hob in a level location. 
3.  Plug your  hob into a standard 220 - 240 volt 13 amp household outlet. 
4.  DO NOT SWITCH THE POWER ON YET - please read the  following WARNINGS & SAFETY PRECAUTIONS first!
WARNINGS & SAFETY PRECAUTIONS.
•	Double check that no packing has been left on the hob.
•	Ensure that the pan you have is ferrous metal (contains iron) You can check your existing pans by using the magnet provided in the box.
•	After long periods of cooking the glass top may become hot.
CONTROLS
The control panel is on the top of the hob closest to the user, The control panel has raised keys. These can be used in helping to orientate the hob. 

Keys from left to right
POWER 					
TEMPERATURE 							
DOWN								
UP 												
TIMER
ON/OFF
OPERATING THE HOB
Make sure there is a compatible pan before you start. If at any point the hob announces “NO PAN” this means that either the pan is not central or it has been removed. Once the pan is located correctly, or put back on the hob, the hob will announce “PAN”, indicating that the connection has been made and cooking may continue.
Select the ON/OFF button on the far right of the hob. The hob will then announce “POWER” to indicate it has turned on. The screen will also display the word ON. You can then place the pan down using the raised white rings to locate the pan in the middle. When you select any function this will be announced. i.e. If you selected the power  button  “ POWER 6” is announced . This is the same for all functions.
Once you have finished cooking then simply press the ON/OFF button and the hob will display the word hot and start an automatic 2 minute cool down period. The hob will also announce  “HOB TEMPERATURE HIGH” every 20 seconds before switching into standby and displaying four dashes - - - -

There are two ways to cook using the induction hob:
POWER COOKING
POWER setting range  1-11
 If the power button is selected then it will announce    “ POWER 6” and the hob will display P6 on the screen. Power 6 is the default setting when the power button is pressed . You can then use the UP or DOWN keys to change the power. The power level chosen depends on the amount of heat you would like, with 1 being the lowest and 11 the highest. 
TEMPERATURE COOKING 
TEMPERATURE setting range 60 degrees C– 280 degrees C.
The process for using the temperature function is done in the same way as that for power. Select the TEMP button and the hob will announce “ TEMPERATURE 160 DEGREES C” and 160 will be displayed on the screen. 160 degrees C is the default setting when TEMP is selected. You can then use the UP or DOWN keys to change the temperature, from 60 degrees C to 280 degrees C.
TIMER
Setting the timer can only be done after either POWER or TEMP has been selected. Once either has been selected you can then press TIMER. The hob will announce  “TIMER”. You can then press the UP and DOWN keys to select how long the timer will run. After three seconds the hob will announce that the timer has started. i.e. “START TIMER”.
The times that can be selected are as follows:
 1 MINUTE			40 MINUTES
2 MINUTES			1 HOUR 
3 MINUTES			1 HOUR AND 20 MINUTES
4 MINUTES 		1 HOUR AND 40 MINUTES
5 MINUTES			2 HOURS 
10 MINUTES 
15 MINUTES 
20 MINUTES 

The timer will then count down automatically and announce the following time remaining during the count down from the maximum of 2 hours.

1 HOUR 			5 MINUTES		40 SECONDS			
50 MINUTES 		4 MINUTES		30 SECONDS				
40 MINUTES		3 MINUTES		20 SECONDS				
30 MINUTES		2 MINUTES		10 SECONDS				
20 MINUTES		1 MINUTE		5 SECONDS			
10 MINUTES		50 SECONDS	FINISHED

When using the TIMER to cook with either POWER or TEMPERATURE, the display will change between the amount of time remaining and the power or temperature that has been set. When cooking with a timer set, you can change the power/temperature level up and down. You can only change the level on the program that was selected prior to setting the timer. i.e. If POWER 6 is selected and you start a 10 MINUTE TIMER, then you can only change the POWER setting up and down. 
Should you press the TIMER key at any point when the timer is counting down, this will turn the TIMER function off.
PROGRAM FINISHED
Once the TIMER has finished, you have ten seconds to select a new program before the automatic cool down period will start. If you want to continue cooking once the automatic cool down has started then the ON/OFF button must be used to turn the hob back on.
CLEANING AND CARE
Ensure that the hob is turned off and has cooled down before cleaning.
Cleaning should be carried out with a damp soapy cloth and surfaces dried afterwards.  Do not use abrasive cleaners on the hob and never pour water over the top.  

NOTE: This appliance should not be used for commercial catering purposes.

ERROR/FAULT CODES

ERROR CODES 		REASON FOR FAULT 
U                                               NO PAN ON THE HOB.OR THE PAN IS 					NOT SUITABLE
F9					GLASS SURFACE SENSOR FAULTY.
F3					CONTROL BOARD SENSOR FAULTY.
E1					ABNORMAL MAINS VOLTAGE HIGH.
E2					ABNORMAL MAINS VOLTAGE LOW.
E3					GLASS SURFACE SENSOR 							OVERHEATED.
E5					CONTROL BOARD SENSOR 							OVERHEATED.
E7					GLASS SURFACE SENSOR FAILED.

SPECIFICATIONS
Power Input 230v AC, 50 Hz
Hob output  1800 Watts (IEC 60705 Rating standard)       
Outside Dimensions 280mm(W) x 65mm(H) x 350mm(D)
Complies with:
EMC Directive 2014/30/EU
LVD Directive  2014/35/EU
ERP Directive  2009/125/EC
Dimensions shown are approximate.
Because we continuously strive to improve our products we may change specifications without prior notice.
Cobolt Systems Ltd
The Old Mill House, 
Mill Road, Reedham,
 Norwich, 
Norfolk
 NR13 3TL
Tel:01493-700172  Fax:01493-701037
Email:sales@cobolt.co.uk
Web:http://www.cobolt.co.uk